- Firmware Update
- Firmware Ver. 2.3
- [HDMI RAW Data Output] can be registered to the Fn buttons

[HDMI RAW Data Output] can be registered to the Fn buttons

[MENU/SET] [] [] [Fn Button Set] Select [Setting in REC mode]

[1] tab [Image Format] [HDMI RAW Data Output] –The menu screen stops being output via HDMI when the [HDMI RAW Data Output] is set to [ON]. Due to this, it is recommended to assign [HDMI RAW Data Output] to a Fn button when you record RAW video by connecting to an external device using HDMI only. [HDMI RAW Data Output] can also be set to [OFF] with the following method: Pressing [MENU/SET], [Q.MENU], and [Fn3] at the same time. ([Info Display (HDMI/SDI)] is switched to [AUTO].)