- 13. Materials
- List of Default Settings / Custom Saving / Settings Available for Copying

List of Default Settings / Custom Saving / Settings Available for Copying

: The function to return to default settings using [Reset].

: The function to save settings details in the Custom mode using [Save to Custom Mode].

: The function to copy settings details using [Save/Restore Camera Setting].

Menu | Default setting | Compatible functions
[Rec Mode]: [Rec Mode] | [Creative Video Mode] |
[Video]: [Image Quality]
[Exposure Mode] | [P] |
[Exposure Comp.] | [±0] |
[Sensitivity] | [AUTO] |
[White Balance] | [AWB] |
[Photo Style] | [] |
[Metering Mode] | [] |
[Dual Native ISO Setting] | [AUTO] |
[ISO Sensitivity (video)] | [ISO Auto Lower Limit Setting] | [160] |
[ISO Auto Upper Limit Setting] | [AUTO] |
[Synchro Scan] | [OFF] |
[Master Pedestal Level] | [0] |
[SS/Gain Operation] | [SEC/ISO] |
[i.Dynamic Range] | [OFF] |
[Vignetting Comp.] | [OFF] |
[Diffraction Compensation] | [OFF] |
[Filter Settings] | [Filter Effect] | [OFF] |
[Video]: [Image Format]
[Rec. File Format] | When [System Frequency] is set to [59.94Hz (NTSC)] or [50.00Hz (PAL)]: [MP4] |
When [System Frequency] is set to [24.00Hz (CINEMA)]: [MOV]
[Image Area of Video] | [FULL] |
[Rec Quality] | When [System Frequency] is set to [59.94Hz (NTSC)]: [FHD/8bit/28M/60p] |
When [System Frequency] is set to [50.00Hz (PAL)]: [FHD/8bit/28M/50p]
When [System Frequency] is set to [24.00Hz (CINEMA)]: [FHD/24p/420/8-L]
[Rec Quality (My List)] | — |
[Variable Frame Rate] | [OFF] |
[Time Code] | [Time Code Display] | [OFF] |
[Count Up] | [REC RUN] |
[Time Code Value] | — | —
[Time Code Mode] | [DF] |
[HDMI Time Code Output] | [OFF] |
[SDI Time Code Output] | [OFF] |
[External TC Setting] | — |
[Genlock] | [Genlock Input] | [OFF] |
[Horizontal Phase Adjustment] | [±0] |
[Luminance Level] | [16-255] |
[Video]: [Focus]
[Focus Mode] | [AF] |
[AF Mode] | [] |
[AF Custom Setting(Video)] | [ON] / [OFF] | [OFF] |
[SET] | — |
[Continuous AF] | [MODE2] |
[Focus Peaking] | [ON] / [OFF] | [ON] |
[SET] | — |
[1-Area AF Moving Speed] | [FAST] |
[Video]: [Audio]
[Sound Rec Level Disp.] | [OFF] |
[Mute Sound Input] | [OFF] |
[Sound Rec Gain Level] | [STANDARD] |
[Sound Rec Level Adj.] | [0dB] |
[Sound Rec Level Limiter] | [ON] |
[Wind Noise Canceller] | [STANDARD] |
[Wind Cut] | [OFF] |
[Lens Noise Cut] | [ON] |
[Mic Socket] | [] |
[Special Mic.] | [Stereo] |
[XLR Mic Adaptor Setting] | [48kHz/16bit] |
[Sound Output] | [REALTIME] |
[Headphone Volume] | [LEVEL3] |
[Video]: [Others]
[Image Stabilizer] | [Operation Mode] | [] |
[E-Stabilization (Video)] | [OFF] |
[Digital Zoom] | [OFF] |
[Focus Transition] | [Start] | — | —
[Focus Pull Setting] | — | —
[Focus Transition Speed] | [M] |
[Focus Transition Rec] | [OFF] |
[Focus Transition Wait] | [OFF] |
[Loop Recording (video)] | [OFF] |
[Segmented File Recording] | [OFF] |
[Live Cropping] | [OFF] |
[Time Stamp Rec.] | [OFF] |
[Custom]: [Image Quality]
[Photo Style Settings] | [Show/Hide Photo Style] | — |
[My Photo Style Settings] | — |
[Reset Photo Style] | — | —
[ISO Increments] | [1/3 EV] |
[Extended ISO] | [OFF] |
[Exposure Offset Adjust.] | [Multi Metering] | [±0 EV] |
[Center Weighted] | [±0 EV] |
[Spot] | [±0 EV] |
[Highlight Weighted] | [±0 EV] |
[Custom]: [Focus/Shutter]
[AF/AE Lock Hold] | [OFF] |
[AF+MF] | [OFF] |
[MF Assist] | (interchangeable lens with a focus ring attached) [Focus Ring] | [ON] |
[AF Mode] | [ON] |
[MF Assist Display] | [PIP] |
[MF Guide] | [ON] |
[Focus Ring Lock] | [OFF] |
[Custom]: [Operation]
[Q.MENU Settings] | [Layout Style] | [MODE1] |
[Item Customize (Video)] | — |
[Fn Button Set] | [Setting in REC mode] | — |
[Setting in PLAY mode] | — |
[Video Rec. Button] | [ON] |
[Custom]: [Monitor / Display]
[Histogram] | [OFF] |
[Focal Length] | [ON] |
[Level Gauge] | [ON] |
[Luminance Spot Meter] | [OFF] |
[Framing Outline] | [OFF] |
[Display Information] | [Display Info in Rec Mode] | [WITH INFO] |
[Display Info in Playback] | [WITH INFO] |
[V-Log L View Assist] | [Read LUT File] | — | —
[LUT Select] | [Vlog_709] |
[LUT View Assist (HDMI)] | [OFF] |
[LUT View Assist (SDI)] | [OFF] |
[HLG View Assist] | [HDMI] | [AUTO] |
[SDI] | [MODE2] |
[Anamorphic Desqueeze Display] | [OFF] |
[Center Marker] | [OFF] |
[Frame Marker] | [ON] / [OFF] | [OFF] |
[SET] | — |
[Zebra Pattern] | [ZEBRA1] / [ZEBRA2] / [ZEBRA1+2] / [OFF] | [OFF] |
[SET] | — |
[Color Bars] | — |
[Red REC Frame Indicator] | [OFF] |
[Custom]: [IN/OUT]
[HDMI Rec Output] | [Down Convert] | [AUTO] |
[HDMI Recording Control] | [OFF] |
[Sound Down Convert] | [OFF] |
[Sound Output (HDMI)] | [ON] |
[HDMI MF Assist Output] | [ON] |
[SDI Rec Output] | [SDI Output Resolution] | When [System Frequency] is set to other than [24.00Hz (CINEMA)]: [1080p] When [System Frequency] is set to [24.00Hz (CINEMA)]: [1080PsF] |
[SDI Recording Control] | [OFF] |
[Sound Output (SDI)] | [ON] |
[SDI Sound Output Gain Adj.] | [-8dB] |
[SDI MF Assist Output] | [ON] |
[Fan Mode] | [AUTO1] |
[Tally Lamp] | [Front Tally Lamp] | [H] |
[Rear Tally Lamp] | [ON] |
[Custom]: [Lens / Others]
[Lens Focus Resume] | [OFF] |
[Power Zoom Lens] | [Step Zoom] | [OFF] |
[Zoom Ring] | [ON] |
[Lens Fn Button Setting] | [Focus Stop] |
[Setup]: [Card/File]
[Card Format] | — | —
[Double Card Slot Function] | [Recording Method] | [] |
[Destination Card Slot] | [] |
[Folder / File Settings] | [Select Folder] | — | —
[Create a New Folder] | — | —
[File Name Setting] | [Folder Number Link] |
[File Number Reset] | — | —
[Copyright Information] | [Artist] | [OFF] |
[Copyright Holder] | [OFF] |
[Display Copyright Info.] | — | —
[Setup]: [Monitor / Display]
[Level Gauge Adjust.] | [Adjust.] | — |
[Level Gauge Value Reset] | — | —
[Setup]: [IN/OUT]
[Headphone Volume] | [LEVEL3] |
[LAN / Wi-Fi] | — | *1
*1Saves the settings of [IP Address Setting (LAN)] in [LAN / Wi-Fi Setup]. However, the IP address set in [Static IP Address Setting] of [IP Address Setting (LAN)] is not saved.
[Bluetooth] | — |
[USB Mode] | [] [PC(Tether)] |
[HDMI / SDI Connections] | [SDI Output] | [ON] |
[Output Resolution(Playback)] | When [SDI Output] is set to [OFF]: [AUTO] When [SDI Output] is set to [ON]: [1080p] (It is [1080PsF] when [System Frequency] is set to [24.00Hz (CINEMA)]) |
[LUT View Assist (HDMI)] | [OFF] |
[HLG View Assist (HDMI)] | [AUTO] |
[LUT View Assist (SDI)] | [OFF] |
[HLG View Assist (SDI)] | [MODE2] |
[Background Color(Playback)] | [] |
[Info Display (HDMI/SDI)] | [AUTO] |
[Power/Network Indicator] | [ON] |
[Card Access Light] | [ON] |
[Setup]: [Setting]
[Save to Custom Mode] | — |
[Load Custom Mode] | — |
[Custom Mode Settings] | [Limit No. of Custom Mode] | [5] |
[Edit Title] | — |
[How to Reload Custom Mode] | — |
[Select Loading Details] | — |
[Save/Restore Camera Setting] | [Save] | — | —
[Load] | — | —
[Delete] | — | —
[Keep Settings While Format] | [OFF] |
[Reset] | — | —
[Setup]: [Others]
[Clock Set] | 2020. 1. 1. 0:00:00 | —
[Time Zone] | GMT +8:00 *1 |
[System Frequency] | [59.94Hz (NTSC)] |
[Device Name] | — |
[Pixel Refresh] | — | —
[Language] | — |
[Firmware Version] | — | —
[Online Manual] | — | —
[My Menu]: [Edit My Menu]
[Add] | — |
[Sorting] | — | —
[Delete] | — | —
[Display from My Menu] | [OFF] |
[Playback] menu: [Playback Mode]
[Anamorphic Desqueeze Display] | [OFF] |
[Playback] menu: [Add/Delete Info.]
[Protect] | — | —
[Rating] | — | —
[Playback] menu: [Edit Image]
[Copy] | — | —
[Playback] menu: [Others]
[Delete All Images] | — | —

*1 The default setting for DC-BGH1GD is “GMT + 9:00”.