- 6. Special Video Recording
- [Synchro Scan]

[Synchro Scan]

Fine-adjust the shutter speed to reduce flickering and horizontal stripes.

The shutter speed set in Synchro Scan is saved separately from the shutter speed used for normal recording. In the Synchro Scan setting screen you can call up the current shutter speed for normal recording and adjust it.

1Set the exposure mode to [S] or [M].

[MENU/SET] [] [] [Exposure Mode] [S] / [M]

2Set [Synchro Scan].

[MENU/SET] [] [] [Synchro Scan] [ON]

3Set the shutter speed.

Rotate to select a numeric value, then press [MENU/SET].

You can call up the current shutter speed for normal recording by pressing [Fn1].

Adjust the shutter speed while looking at the screen so that flickering and horizontal stripes will be minimized.

When you set [Synchro Scan] to [ON], the available shutter speed range becomes narrower.