- 5. Recording settings
- Metering / Exposure / ISO Sensitivity
- [Dual Native ISO Setting]

[Dual Native ISO Setting]

You can set whether to switch the base sensitivity automatically or to fix it.

[MENU/SET] [] [] Select [Dual Native ISO Setting]

[AUTO] | The base sensitivity is automatically switched according to the brightness. ISO sensitivity that can be set: [AUTO] / [160] to [51200]. (When [Extended ISO] is set: [AUTO] / [80] to [204800].)
[LOW] | Sets the base sensitivity for low sensitivity. ISO sensitivity that can be set: [AUTO] / [160] to [800]. (When [Extended ISO] is set: [AUTO] / [80] to [800].)
[HIGH] | Sets the base sensitivity for high sensitivity. ISO sensitivity that can be set: [AUTO] / [800] to [51200]. (When [Extended ISO] is set: [AUTO] / [800] to [204800].)

When [Filter Settings] is set to [High Dynamic], [Dual Native ISO Setting] is fixed to [AUTO].