- 11. Menu Guide
- [Setup] menu
- [Setup] menu ([Others])

[Setup] menu ([Others])

: Default settings

[Clock Set]

Sets the date and time. (Clock Set)

[Time Zone]

Sets the time zone. (Time zone)

[System Frequency]

[59.94Hz (NTSC)] / [50.00Hz (PAL)] / [24.00Hz (CINEMA)]
This changes the system frequency of videos that are recorded and played back. ([System Frequency])

[Device Name]

This will set the camera name (32 characters or less). For information on how to enter characters (Entering Characters) The set name will be displayed as the individual ID for SSID during Wi-Fi connection or Tethered recording. When Tethered recording using several cameras, it is recommended to set an individual device name for each camera.

[Pixel Refresh]

This optimizes the image sensor and image processing. The image sensor and image processing are optimized when the camera is purchased. Use this function when bright spots that do not exist in the subject get recorded. When performing pixel refresh, block the lens from light with a body cap etc. Turn the camera off and on after the pixels are corrected.

[Language]

This set the language displayed on the screen. If you set a different language by mistake, select [] from the menu icons to set the desired language.

[Firmware Version]

[Firmware Update] / [Software info]
You can check the firmware versions of the camera and lens. In addition, you can update the firmware, and display information about the camera software. [Firmware Update]: Updates firmware. 1Download the firmware. (Firmware of Your Camera/Lens) 2Save the firmware to the root directory of the card (the first folder that appears when you access the card on your PC), and then insert the card into the camera. 3Select [Firmware Update], press [MENU/SET], and then select [Yes] to update the firmware. [Software info]: Displays information about the camera software. When a supported optional item (XLR Microphone Adaptor, etc.) is attached to the camera, you can also check its firmware version.

[Online Manual]

[URL display] / [QR Code display]
Displays the URL or QR code in order to browse the “Operating Instructions” (HTML/PDF).