- 5. Recording settings
- Main Assist Functions
- [SS/Gain Operation]

[SS/Gain Operation]

You can switch the units of shutter speed values and gain (sensitivity) values.

[MENU/SET] [] [] Select [SS/Gain Operation]

[SEC/ISO] | Displays the shutter speed in seconds and the gain in ISO.
[ANGLE/ISO] | Displays the shutter speed in degrees and the gain in ISO. The angle can be set in a range between 11° and 358°. (When [Synchro Scan] is set to [OFF])
[SEC/dB] | Displays the shutter speed in seconds and the gain in dB. 0 dB corresponds to either of the following ISO sensitivity values. –When [Dual Native Gain Setting] is set to [AUTO] or [LOW]: [160] –When [Dual Native Gain Setting] is set to [HIGH]: [800]

When [SS/Gain Operation] is set to [SEC/dB], menu names change as shown below:

–[Dual Native ISO Setting] [Dual Native Gain Setting]

–[ISO Sensitivity (video)] [Gain Setting]

–[ISO Auto Lower Limit Setting] [Auto Gain Lower Limit Setting]

–[ISO Auto Upper Limit Setting] [Auto Gain Upper Limit Setting]

–[Extended ISO] [Extended Gain Setting]

Setting Range for Gain (Sensitivity)

When [SS/Gain Operation] is set to [SEC/dB], gain (sensitivity) can be set in the following ranges.

[Dual Native Gain Setting] | [Extended Gain Setting] | Setting Range for Gain (Sensitivity)
[AUTO] | [OFF] | [AUTO], [0 dB] to [50 dB]
[ON] | [AUTO], [–6 dB] to [62 dB]
[LOW] | [OFF] | [AUTO], [0 dB] to [14 dB]
[ON] | [AUTO], [–6 dB] to [14 dB]
[HIGH] | [OFF] | [AUTO], [0 dB] to [36 dB]
[ON] | [AUTO], [0 dB] to [48 dB]