- Firmware Update
- Firmware Ver. 2.5
- [Operation Lock Setup]

[Operation Lock Setup]

Sets the operations to be disabled with the Fn button [Operation Lock]. (Only for recording screen)

[MENU/SET] [] [] Select [Operation Lock Setup]

: Default settings

[] (Playback) button | /
[Q.MENU] button | /
[] (Delete) button / [] (Cancel) button | /
Cursor buttons / [MENU/SET] button | /
Control dial | /
Video rec. button | /
Fn button (Fn1) | /
Fn button (Fn2) | /
Fn button (Fn3) | /
Fn button (Fn4) | /
Lens | /
Each press of [MENU/SET] switches between “Lock” and “Unlock”. Press [Fn1] to change the page. Press [Q.MENU] to return to the default settings. When you operate locked operation parts, [] is displayed on the screen. The operation parts to be locked by “Lens” differ depending on the lens. The lens switch will not be locked. Depending on the lens you use, [] may not be displayed on the screen even if you operate the lens when it is locked in “Lens”. After setting the lock by “Lens”, check whether it is locked by actually operating it. A Fn button registered with [Operation Lock] by the [Fn Button Set] will not be locked even if it is set to [].