- 5. Recording settings
- White Balance / Image Quality
- [Filter Settings]

[Filter Settings]

This mode records with additional image effects (filters).

1Set the [Filter Effect].

[MENU/SET] [] [] [Filter Settings] [Filter Effect] [SET]

2Select the filter.

Press to select, and then press [MENU/SET].

Press [Fn1] to switch the screen between normal display and guide display.

The guide display shows the description of each filter.

Adjusting the Filter Effect

You can adjust the filter effect.

Select the filter.

On the recording screen, press .

Rotate to set.

To return to the recording screen, press [MENU/SET] again.

When the filter effect is adjusted, the filter icon on the recording screen is indicated with [].

Filter | Items that can be adjusted
[Expressive] | Vividness
[Retro] | Coloring
[Old Days] | Contrast
[High Key] | Coloring
[Low Key] | Coloring
[Sepia] | Contrast
[Monochrome] | Coloring
[Dynamic Monochrome] | Contrast
[Impressive Art] | Vividness
[High Dynamic] | Vividness
[Cross Process] | Coloring
[Toy Effect] | Coloring
[Toy Pop] | Area with reduced peripheral brightness
[Bleach Bypass] | Contrast
[Miniature Effect] | Vividness
[Fantasy] | Vividness
[One Point Color] | Amount of color left

White balance will be fixed to [AWB].

The upper limit to ISO sensitivity is [6400].

When [High Dynamic] is set, the ISO sensitivity is fixed to [AUTO].

Depending on the filter, the recording screen may seem as if frames are missed.

When [Image Area of Video] is [PIXEL/PIXEL], recording video with [Toy Effect] / [Toy Pop] is not possible.

Filter on/off operations can be registered to a Fn button:

[] [] [Fn Button Set] [Setting in REC mode] [Filter Effect] (Register Functions to the Fn Buttons)

When displaying the [Filter Effect] setting screen using the Fn button, pressing [Fn1] displays the filter selection screen.

Setting the Type of Defocus ([Miniature Effect])

Set [Filter Effect] to [Miniature Effect].

Press to display the setting screen.

Press or to move the in-focus portion.

Rotate to change the size of in-focus portion.

To reset the in-focus portion setting to the default, press [Fn1].

Press [MENU/SET] to set.

No audio is recorded in videos.

When the system frequency is set to [59.94Hz (NTSC)], the length of the video recorded will be approx. 1/10 of the actual recording time. The displayed video recording time will be approx. 10 times longer than the recording time displayed during normal video recording.

When the system frequency is set to [50.00Hz (PAL)] or [24.00Hz (CINEMA)], the length of the video recorded will be approx. 1/8 of the actual recording time. The displayed video recording time will be approx. 8 times longer than the recording time displayed during normal video recording.

If you end video recording after a short time, the camera may go on recording for a certain period.

Setting the Color to Be Left ([One Point Color])

Set [Filter Effect] to [One Point Color].

Press to display the setting screen.

Press to move the frame and select the color you want to leave.

To return the frame back to the center, press [Fn1].

Press [MENU/SET].