- 7. Output image
- SDI output settings
- Set the resolution during recording when output via SDI

Set the resolution during recording when output via SDI

Set the resolution of the image to be output via SDI.

[MENU/SET] [] [] [SDI Rec Output] Select [SDI Output Resolution]

Settings: [1080p] / [1080i] / [1080PsF] / [720p]

Settings Items ([SDI Output Resolution])

Output is with the resolution and frame rate according to the combinations of the [Rec Quality] and [SDI Output Resolution] settings.

The items that can be set at [SDI Output Resolution] differs depending on the recording frame rate of the [Rec Quality].

[System Frequency]: [59.94Hz (NTSC)]

[SDI Output Resolution] | Recording frame rate of the [Rec Quality]
59.94p | 29.97p | 23.98p
1080p | 1080/59.94p | 1080/29.97p | 1080/23.98p
1080i | 1080/59.94i | — | —
1080PsF | — | 1080/29.97PsF | 1080/23.98PsF
720p | 720/59.94p | — | —

[System Frequency]: [50.00Hz (PAL)]

[SDI Output Resolution] | Recording frame rate of the [Rec Quality]
50.00p | 25.00p
1080p | 1080/50.00p | 1080/25.00p
1080i | 1080/50.00i | —
1080PsF | — | 1080/25.00PsF
720p | 720/50.00p | —

[System Frequency]: [24.00Hz (CINEMA)]

[SDI Output Resolution] | Recording frame rate of the [Rec Quality]
24.00p
1080p | —
1080i | —
1080PsF | 1080/24.00PsF
720p | —

This memorizes the setting value for each recording frame rate of [Rec Quality].

When [System Frequency] is set to [24.00Hz (CINEMA)], it is fixed to [1080PsF].