- 5. Recording settings
- Metering / Exposure / ISO Sensitivity
- [ISO Sensitivity (video)]

[ISO Sensitivity (video)]

Sets the lower and upper limits for ISO sensitivity when ISO sensitivity is set to [AUTO].

[MENU/SET] [] [] Select [ISO Sensitivity (video)]

[ISO Auto Lower Limit Setting] | Sets the lower limit for ISO sensitivity when ISO sensitivity is [AUTO]. Set in the range between [160] and [25600].
[ISO Auto Upper Limit Setting] | Sets the upper limit for ISO sensitivity when ISO sensitivity is [AUTO]. Set to [AUTO] or in the range between [200] and [51200].

When [Filter Settings] is set to [High Dynamic], [ISO Sensitivity (video)] cannot be used.