- 13. Materials
- Specifications

Specifications

The specifications are subject to change for performance enhancement.

It is possible to record photos (still images) using software “LUMIX Tether”.

Digital camera body (DC-BGH1):

Information for your safety

Power source: 12 V Power consumption: 7.9 W (when recording), 6.7 W (when playing back) [When the interchangeable lens H-ES12060 is attached.]

Type

Type | Digital Single Lens Mirrorless camera
Recording media | SD memory card / SDHC memory card*1 / SDXC memory card*1 *1Compliant with UHS-I/UHS-II UHS Speed Class 3, UHS-II Video Speed Class 90 Double slot recording function is available.
Lens mount | Micro Four Thirds mount

Image sensor

Image sensor | 4/3″ Live MOS sensor, a total of 11,930,000 pixels, primary color filter
Effective number of pixels of the camera | 10,280,000 pixels

Latitude

13 stops ([V-Log L])

Recording format for video

Video format | MP4 (H.264/MPEG-4 AVC, H.265/HEVC) MOV (H.264/MPEG-4 AVC, H.265/HEVC)
Audio format | MP4: AAC (2ch) MOV: LPCM (2ch, 48 kHz/16 bit)*2 *2When an XLR Microphone Adaptor (DMW-XLR1: optional) is attached, LPCM (2ch, 48 kHz/24-bit, 96 kHz/24-bit) can be selected
Image quality for video | Refer to [Rec Quality] in this document. ([Rec Quality])

Recording format for still images

File format for still images | JPEG (DCF compliant, Exif 2.31 compliant)
Image size (pixels) | L: 3680×2760 M: 2592×1944 S: 1824×1368 (The aspect ratio is fixed to [4:3].)
Image quality for photos | Fine / Standard

Focus

AF type | TTL type based on image detection (Contrast AF)
Focus mode | AF / MF
AF mode | Automatic detection (Face/Eye/Body/Animal) / Tracking (only for video) / 225-Area / Zone (Oval) (only for video) / 1-Area

Exposure control

Light metering system, Light metering mode | 1728-zone metering, multi-metering / center-weighted metering / spot metering / highlight-weighted metering (only for video)
Metering range | EV 0 to EV 18 (F2.0 lens, ISO100 conversion)
Exposure | Program AE (P) / Aperture-Priority AE (A) / Shutter-Priority AE (S) / Manual Exposure (M)
Exposure compensation | 1/3 EV steps, ±3 EV (Videos), ±5 EV (Photos)
ISO sensitivity (standard output sensitivity) | AUTO / 160 to 51200, When [Extended ISO] is set: AUTO / 80 to 204800, 1/3 EV steps
Dual Native ISO setting | Auto Base sensitivity: 160/800 (dB display values are based on 160) AUTO / 160 to 51200 When [Extended ISO] is set: AUTO / 80 to 204800 Low sensitivity Base sensitivity: 160 AUTO / 160 to 800 When [Extended ISO] is set: AUTO / 80 to 800 High sensitivity Base sensitivity: 800 AUTO / 800 to 51200 When [Extended ISO] is set: AUTO / 800 to 204800
Dual Native ISO setting ([V-Log L]) | Auto Base sensitivity: 400/2000 (dB display values are based on 400) AUTO / 400 to 25600 Low sensitivity Base sensitivity: 400 AUTO / 400 to 2000 High sensitivity Base sensitivity: 2000 AUTO / 2000 to 25600
Dual Native ISO setting ([Hybrid Log Gamma]) | Auto Base sensitivity: 320/1600 (dB display values are based on 320) AUTO / 320 to 51200 When [Extended ISO] is set: AUTO / 320 to 204800 Low sensitivity Base sensitivity: 320 AUTO / 320 to 1600 High sensitivity Base sensitivity: 1600 AUTO / 1600 to 51200 When [Extended ISO] is set: AUTO / 1600 to 204800

White balance

AWB / AWBc / AWBw / Daylight / Cloudy / Shade / Incandescent lights / White set 1, 2, 3, 4 / Color temperature 1, 2, 3, 4

Shutter

Shutter speed | Videos: 1/2 of a second to 1/16000 of a second Photos: 1 second to 1/16000 of a second

Zoom

Digital Zoom | 2x / 4x

Microphone

Stereo

Interface

[REMOTE] | Ø2.5 mm jack Terminal for generic remote control unit (A Panasonic shutter remote control (DMW-RS2) cannot be used.)
[DC IN 12 V] | DC 12 V (11.4 V to 12.6 V), EIAJ Type 4
[MIC] | Ø3.5 mm stereo mini jack
Headphones | Ø3.5 mm stereo mini jack
LAN connector | LAN terminal (RJ-45) for remote control×1, compatible with power supply by PoE+ (IEEE 802.3at compliant) Use an IEC60950-1 or IEC62368-1 compliant PoE+ (IEEE 802.3at compliant) switching hub or power supplying device.
[SDI OUT] | BNC terminal×1, 0.8 V [p-p], 75 Ω, 3G-SDI Level-A / HD-SDI compatible
[TC IN/OUT] | BNC terminal×1
[GENLOCK IN] | BNC terminal×1, BBS (Black Burst sync) signal and tri-level sync signal compatible
HDMI | HDMI Type A
USB | USB Type-C™, SuperSpeed USB3.1 GEN1

External dimensions / Mass

External dimensions | Approx. 93.0 mm (W)×93.0 mm (H)×78.0 mm (D) (3.66″ (W)×3.66″ (H)×3.07″ (D)) (excluding the projecting parts)
Mass (Weight) | Approx. 545 / 1.2 lb (only camera body)

Operating environment

Recommended operating temperature | -10 °C to 40 °C (14 °F to 104 °F) Battery performance temporarily worsens at low temperatures (-10 °C to 0 °C (14 °F to 32 °F)), reducing the available recording time.
Permissible relative humidity | 10%RH to 80%RH

Wi-Fi

Compliance standard | IEEE 802.11b/g/n (standard wireless LAN protocol)
Frequency range used (central frequency) | 2412 MHz to 2462 MHz (1 to 11 ch)
Encryption method | Wi-Fi compliant WPA™/WPA2™
Access method | Infrastructure mode

Bluetooth

Compliance standard | Bluetooth Ver. 4.2 (Bluetooth Low Energy (BLE))
Frequency range used (central frequency) | 2402 MHz to 2480 MHz

AC adaptor (Panasonic SAE0011A):

Information for your safety

Input: 100 V - 240 V 50/60 Hz 1.2 A 79 VA (100 V ) - 99 VA (240 V ) Output: 12 V 3.0 A

The symbols on this product (including the accessories) represent the following:

AC DC Class II equipment (The construction of the product is double-insulated.) ON Stand-by

This camera complies with the “Design rule for Camera File system” (DCF) and “Exchangeable Image File Format” (Exif) standards established by “Japan Electronics and Information Technology Industries Association” (JEITA). The camera cannot playback files that do not comply with the DCF standard. Exif is a file format for still images which allows recording information, etc. to be added.