- 11. Menu Guide
- [Custom] menu
- [Custom] menu ([Image Quality])

[Custom] menu ([Image Quality])

: Default settings

[Photo Style Settings]

[Show/Hide Photo Style] | [Vivid] / [Natural] / [Landscape] / [Portrait] / [L.Monochrome] / [L.Monochrome D] / [Cinelike D2] / [Cinelike V2] / [Like709] / [V-Log L] / [Hybrid Log Gamma] / [MY PHOTO STYLE 1] to [MY PHOTO STYLE 10]
Sets Photo Style items to be displayed on the menu.
[My Photo Style Settings] | [Add Effects]
[Load Preset Setting]
Enables detailed image quality adjustment settings for My Photo Style. [Add Effects]: Enables [Dual Native ISO Setting], [Sensitivity], and [White Balance] settings in image quality adjustment. [Load Preset Setting]: Sets the timing at which image quality adjustment values changed in My Photo Style are returned to their registered state.
[Reset Photo Style]
Returns details changed in [Photo Style] and [Photo Style Settings] to their default settings.

[ISO Increments]

[1/3 EV] / [1 EV]
Changes the intervals between ISO sensitivity adjustment values.

[Extended ISO]

[ON] / [OFF]
Extends the setting range of ISO sensitivity. The extendible range depends on the [Dual Native ISO Setting] ([Dual Native ISO Setting]). –When set to [AUTO]: Lower limit can be extended to [80] and the upper limit can be extended to [204800] –When set to [LOW]: Lower limit can be extended to [80] –When set to [HIGH]: Upper limit can be extended to [204800]

[Exposure Offset Adjust.]

[Multi Metering] | [-1 EV] to [+1 EV] ( [±0 EV])
[Center Weighted] | [-1 EV] to [+1 EV] ( [±0 EV])
[Spot] | [-1 EV] to [+1 EV] ( [±0 EV])
[Highlight Weighted] | [-1 EV] to [+1 EV] ( [±0 EV])
Adjusts the exposure level that is the standard correct exposure for each item of [Metering Mode]. Adds the adjustment value from this function to the exposure compensation value (Exposure Compensation) when recording. It is not possible to add an adjustment value of a range that exceeds ±3 EV.