- 13. Materials
- Lamp / Indicator Display

Lamp / Indicator Display

Shows the status of the camera with the lamp/indicator.

Status indicator (Green / Orange)

Lights up (Green) | The camera is turned on.
Lights up (Orange) | Tether connect mode (Tether Connection Mode)
Blinks (Green, once/sec.) | (When using PoE+ power supply.) Determining PoE+. (Supplying power from a PoE+ power supply) (When using battery.) Low battery (It blinks in orange when in Tether connect mode.)
Blinks (Green, 4 times/sec.) | (When using PoE+ power supply.) Insufficient power supply capacity (When using battery.) The camera is turned off forcibly due to low battery. (It blinks in orange when in Tether connect mode.)
Blinks (alternately green and orange) | System error (Turn off the camera and then on again.)
Off | The camera is turned off.

Front tally lamp / Rear tally lamp (Red)

Lights up | During video recording. (or sending data to external devices)
Blinks (Red, once/sec.) | Low battery and card capacity.
Blinks (Red, 4 times/sec.) | Stops recording forcibly due to low battery and card capacity.

[NETWORK] connection lamp (Blue)

Lights up | After being connected with a LAN cable. When Wi-Fi/Bluetooth function is ON or connected.
Blinks | When sending Tether recorded images to a PC from a camera.

When the power is turned off and [Remote Wakeup] is set to [ON], the [NETWORK] connection lamp turns off even if the Bluetooth function is working.