- 7. Output image
- Images Output via HDMI

Images Output via HDMI

Aspect ratio, resolution, and frame rate output is according to the [Rec Quality] settings in the [Video] ([Image Format]) menu. Resolution and frame rate can be down-converted for output according to the application. YUV 4:2:2 is used for YUV and bit value output, as shown below.

Recording to card | HDMI output
4:2:2 10 bit | 4:2:2 10 bit
4:2:0 10 bit | 4:2:2 10 bit
4:2:0 8 bit | 4:2:2 8 bit

Resolution, frame rate

Resolution and frame rate is output according to the following menu combinations:

–[Rec Quality] in the [Video] ([Image Format]) menu.

–[Down Convert] in [HDMI Rec Output] of the [Custom] ([IN/OUT]) menu.

Anamorphic (4:3) video is output with a 4K or FHD resolution.

For details, refer to “Image Quality When Outputting via HDMI”. (Image Quality When Outputting via HDMI)

When set to a 4:3 [Rec Quality], bands are added to the images and they are output with a 16:9 aspect ratio.

Output may be in 8-bit if you output to devices that do not support 10-bit.

Notice Regarding HDMI Output

It may take some time for the output method to change.

When you use the HDMI output during recording, the image may be displayed with a time lag.

When you check the image and audio from the external device connected to the camera, the microphone of the camera may pick up the sound from the speakers of the external device, producing an abnormal sound (audio feedback). If this occurs, move the camera away from the external device or lower the volume on the external device.