- 5. Recording settings
- Main Assist Functions
- [Luminance Spot Meter]

[Luminance Spot Meter]

Specify any spot on the subject to measure the luminance over a small area.

1Set [Luminance Spot Meter].

[MENU/SET] [] [] [Luminance Spot Meter] [ON]

2Select the position where you want to measure the luminance.

Press to select and then press [MENU/SET].

To return the position back to the center, press [Fn1].

Measurement Range

Measuring is possible in the range –7% to 109% (IRE).

When [Photo Style] is set to [V-Log L], this can be measured with Stop units. (Calculated as 0 Stop=42% (IRE))