- 5. Recording settings
- Metering / Exposure / ISO Sensitivity
- ISO Sensitivity

ISO Sensitivity

You can set light sensitivity (ISO sensitivity). With the default settings, you can set 160 to 51200 in 1/3 EV increments. This camera supports Dual Native ISO which enables recording at high sensitivity with reduced noise by switching the base sensitivity. The base sensitivity can also be fixed as necessary.

1Press [Fn3].

At default setting, [Sensitivity] is assigned to [Fn3].

About Fn buttons (Fn Buttons)

You can also set it in the [Sensitivity] of the [Video] ([Image Quality]) menu

2Select ISO sensitivity.

Rotate .

3Confirm your selection.

Press [MENU/SET].

Setting Items (ISO Sensitivity)

[AUTO] | The ISO sensitivity is automatically adjusted according to the brightness. Maximum [6400]*1
[160] to [51200] | The ISO sensitivity is fixed at the selected value. You can extend the ISO sensitivity range in between a lower limit of [80] and an upper limit of [204800] by setting [Extended ISO] ([Extended ISO]) to [ON] in the [Custom] ([Image Quality]) menu.

*1Default setting. The upper limit can be changed with [ISO Sensitivity (video)].

When the following functions are being used, the ISO sensitivity that can be set is restricted.

–[High Dynamic] ([Filter Settings]): Fixed to [AUTO]

–Other than [High Dynamic] ([Filter Settings]): Up to an upper limit of [6400]

–[Like709] ([Photo Style]): Down to a lower limit of [160]

–[V-Log L] ([Photo Style]): Down to a lower limit of [400], up to an upper limit of [25600]

–[Hybrid Log Gamma] ([Photo Style]): Down to a lower limit of [320].

You can change the intervals between ISO sensitivity settings values:

[] [] [ISO Increments] ([ISO Increments])

The setting range of ISO sensitivity can be extended:

[] [] [Extended ISO] ([Extended ISO])

You can change the units for sensitivity to dB when recording video:

[] [] [SS/Gain Operation] ([SS/Gain Operation])