- 11. Menu Guide
- [Video] menu
- [Video] menu ([Image Quality])

[Video] menu ([Image Quality])

: Default settings

[Exposure Mode]

[P] / [A] / [S] / [M]
Sets the exposure mode. ([Exposure Mode])

[Exposure Comp.]

[-3] to [+3] ( ± 0)
This compensates the exposure. (Exposure Compensation)

[Sensitivity]

[AUTO] / [160] to [51200]
This sets the sensitivity to light. (ISO Sensitivity)

[White Balance]

[AWB] / [AWBc] / [AWBw] / [] / [] / [] / [] / [] to [] / [] to []
This compensates the effect of the light of the color that illuminates the subject. (White Balance (WB))

[Photo Style]

[Standard] / [Vivid] / [Natural] / [Landscape] / [Portrait] / [Monochrome] / [L.Monochrome] / [L.Monochrome D] / [Cinelike D2] / [Cinelike V2] / [Like709] / [V-Log L] / [Hybrid Log Gamma] / [MY PHOTO STYLE 1] to [MY PHOTO STYLE 10]
You can select the finishing settings of images to suit your subjects and expression styles. ([Photo Style])

[Metering Mode]

[] / [] / [] / []
You can switch the method of measurement for the brightness. ([Metering Mode])

[Dual Native ISO Setting]

[AUTO] / [LOW] / [HIGH]
Sets whether to switch the base sensitivity automatically or to fix it. ([Dual Native ISO Setting])

[ISO Sensitivity (video)]

[ISO Auto Lower Limit Setting] | [160] to [25600]
[ISO Auto Upper Limit Setting] | [AUTO] / [200] to [51200]
Sets the lower and upper limits for ISO sensitivity when ISO sensitivity is set to [AUTO]. ([ISO Sensitivity (video)])

[Synchro Scan]

[ON] / [OFF]
Fine-adjust the shutter speed to reduce flickering and horizontal stripes. ([Synchro Scan])

[Master Pedestal Level]

[-15] to [15] ( 0)
You can adjust the black level, which serves as the reference for images. ([Master Pedestal Level])

[SS/Gain Operation]

[SEC/ISO] / [ANGLE/ISO] / [SEC/dB]
You can switch the units of shutter speed values and gain (sensitivity) values. ([SS/Gain Operation])

[i.Dynamic Range]

[AUTO] / [HIGH] / [STANDARD] / [LOW] / [OFF]
Contrast and exposure are compensated when the brightness difference between the background and subject is great. Compensation effect may not be achieved depending on the recording conditions. When the following functions are being used, [i.Dynamic Range] is not available: –[Like709] / [V-Log L] / [Hybrid Log Gamma] ([Photo Style]) –[Filter Settings]

[Vignetting Comp.]

[ON] / [OFF]
When the screen periphery darkens as a result of the lens characteristics, you can record pictures with the brightness of the screen periphery corrected. Compensation effect may not be achieved depending on the recording conditions. Noise in the periphery of the picture may stand out with higher ISO sensitivity. When the following functions are being used, [Vignetting Comp.] is not available: –[PIXEL/PIXEL] ([Image Area of Video]) –[Variable Frame Rate]

[Diffraction Compensation]

[AUTO] / [OFF]
The camera raises the image resolution by correcting the blurriness caused by diffraction when the aperture is closed. Compensation effect may not be achieved depending on the recording conditions. Noise may stand out with higher ISO sensitivity.

[Filter Settings]

[Filter Effect] | [ON] / [OFF] / [SET]
This mode records with additional image effects (filters). ([Filter Settings])