- 11. Menu Guide
- [Custom] menu
- [Custom] menu ([Focus/Shutter])

[Custom] menu ([Focus/Shutter])

: Default settings

[AF/AE Lock Hold]

[ON] / [OFF]
This sets button operations for AF/AE Lock. Turning this [ON] maintains the lock after releasing the button until it is pressed again.

[AF+MF]

[ON] / [OFF]
You can fine-adjust the focus manually during AF Lock by rotating the focus ring. –When a Fn button that has [AF-ON] registered is pressed –When locked using the Fn button [AF LOCK] or [AF/AE LOCK]

[MF Assist]

(When an interchangeable lens with a focus ring is attached) [Focus Ring] | [ON] / [OFF]
[AF Mode] | [ON] / [OFF]
[MF Assist Display] | [FULL] / [PIP]
This sets the display method of MF Assist (enlarged screen). [Focus Ring]: The screen is enlarged by focusing with the lens. [AF Mode]: The screen is enlarged by pressing a Fn button that has [AF Mode] registered. [MF Assist Display]: Sets the display method (full screen mode/windowed mode) of MF Assist (enlarged screen). While you are using the following functions, MF Assist will not be displayed: –Video recording –[Digital Zoom]

[MF Guide]

[ON] / [OFF]
During MF, MF Guide, which acts as a guide to recording distance, is displayed on the screen.

[Focus Ring Lock]

[ON] / [OFF]
This disables the focus ring operation during MF to lock the focus. [MFL] is displayed on the recording screen while the focus ring is locked.