- 6. Special Video Recording
- Log Recording
- [V-Log L View Assist]

[V-Log L View Assist]

When [Photo Style] is set to [V-Log L], images output via HDMI/SDI will darken. Using [V-Log L View Assist] means you can output images with LUT data applied via HDMI/SDI.

[MENU/SET] [] [] Select [V-Log L View Assist]

[Read LUT File] | Reads LUT data from the card.
[LUT Select] | Selects the LUT data to be applied from among the preset ([Vlog_709]) and registered LUT data.
[LUT View Assist (HDMI)] | Applies LUT data to images output over HDMI.
[LUT View Assist (SDI)] | Applies LUT data to images output over SDI.

When applying the LUT data, [LUT] is displayed on the recording screen.

Up to 4 LUT data files can be registered.

Reading LUT Files

The following LUT data can be used: –The “.vlt” format, which meets the requirements specified in the “VARICAM 3DLUT REFERENCE MANUAL Rev.1.0” –File names consisting of up to 8 alphanumeric characters (excluding extension) Save the LUT data with a file extension of “.vlt” in the root directory of the card (the folder opened when the card is opened on a PC).

Insert a card on which LUT data is saved into the camera.

Select [Read LUT File].

[MENU/SET] [] [] [V-Log L View Assist] [Read LUT File] [Card Slot 1] / [Card Slot 2]

Press to select the LUT data to read and then press [MENU/SET].

Press to select the location to register the data, and then press [MENU/SET].

When registered items are selected, they will be overwritten.