- Firmware Update
- Firmware Ver. 2.5
- [LUT View Assist (Tether)]

[LUT View Assist (Tether)]

When [Photo Style] is set to [V-Log L], images output via external device will be displayed darker.

When [LUT View Assist (Tether)] in [V-Log L View Assist] is set, the image applied with LUT data can be output via “LUMIX Tether”/“LUMIX Sync”.

[MENU/SET] [] [] [V-Log L View Assist] Select [LUT View Assist (Tether)]

[ON] | Outputs the image applied with LUT data to “LUMIX Tether”/“LUMIX Sync”.
[OFF] | Outputs the image to “LUMIX Tether”/“LUMIX Sync” without applying LUT data.

You can register [LUT View Assist (Tether)] to [Fn Button Set]/[Q.MENU Settings].