- 5. Recording settings
- Metering / Exposure / ISO Sensitivity
- [Metering Mode]

[Metering Mode]

The type of optical measurement to measure brightness can be changed.

[MENU/SET] [] [] Select [Metering Mode]

(Multi-metering) | Method in which the most suitable exposure is measured by judging the allocation of brightness on the whole screen.
(Center-weighted) | Method used to perform measuring which focuses on the center of the screen.
(Spot) | Method used to measure the extremely small part around the spot-metering target. When you move the AF area, the spot metering target also moves to match. Spot-metering target
(Highlight-weighted) | Method used to perform measuring which focuses on the highlighted parts of the screen to prevent overexposure. This is suitable for theater photography, etc.

The standard value for correct exposure can be adjusted:

[] [] [Exposure Offset Adjust.] ([Exposure Offset Adjust.])