- 12. Remote Operations
- [LAN / Wi-Fi Setup] menu

[LAN / Wi-Fi Setup] menu

This configures the settings required for the wired LAN / Wi-Fi function. The settings cannot be changed when connected to wired LAN / Wi-Fi.

1Displaying the [LAN / Wi-Fi Setup] menu.

[MENU/SET] [] [] [LAN / Wi-Fi] [LAN / Wi-Fi Setup]

Cannot be set during connection via USB.

[IP Address Setting (LAN)] | Set the IP address for wired LAN connection. You can select whether to automatically assign an IP address using a DHCP or to set any fixed IP address. [DHCP Server]: Select this to connect the camera as a DHCP server (default setting). [DHCP Client]: Select this to connect the camera as a DHCP client. [Static IP Address]: Select this to connect using the IP address set in [Static IP Address Setting]. [Static IP Address Setting]: You can set IP address used for [Static IP Address]. [IP Address]: The default setting is <192.168.0.2>. [Subnet Mask]: The default setting is <255.255.255.0>. [Default Gateway]: The default setting is <192.168.0.1>. Set the IP address, subnet mask, and default gateway with the correct combination. For details about DHCP settings or settings of a fixed IP address, contact the administrator of the network you are using. If you changed the setting of [IP Address Setting (LAN)], turn the camera off and then on again.
[Wi-Fi Password] | You can use a password to connect for enhanced security. (Using Password Authentication to Connect)
[LAN / Wi-Fi Function Lock] | To prevent incorrect operation and use of the wired LAN / Wi-Fi function by a third party and to protect personal information in the camera and included with images, protect the wired LAN / Wi-Fi function with a password. [Setup]: Enter any 4-digit numbers as the password. For information on how to enter characters (Entering Characters) [Cancel]: Cancel the password. Once a password is set, you are required to enter it each time you use the wired LAN / Wi-Fi function. If you forget your password, you can use [Reset] in the [Setup] ([Setting]) menu to reset the network settings and thereby reset the password.
[Network Address Display (LAN)] | Displays the MAC address and IP address of the camera during wired LAN connection.
[Network Address Display (Wi-Fi)] | Displays the MAC address and IP address of the camera during Wi-Fi connection.