- 2. Getting Started
- Inserting Cards (Optional)
- [Double Card Slot Function]

[Double Card Slot Function]

This sets the way recording to the card slots 1 and 2 is performed.

[MENU/SET] [] [] Select [Double Card Slot Function]

[Recording Method] | ([Relay Rec]) | Selects the priority of card slots for recording. [Destination Card Slot]: [] / [] Relays recording to the card in the other card slot after the first card runs out of free space.
([Backup Rec]) | Records the same images to both cards simultaneously.
([Allocation Rec]) | Allows you to specify the card slot to be used for recording for different image formats. [JPEG Destination]*1 / [Video Destination]

*1You can use it when recording still images using the “LUMIX Tether” software.

Notes about relay recording

The following video cannot be continued to be recorded on another card:

–[Loop Recording (video)]

Notes about Backup Recording

We recommend using cards with the same Speed Class rating and capacity.

If the card Speed Class or capacity is insufficient when video recording, recording to both cards stops.

Backup recording is not available with the following video. They can only be recorded on a single card:

–[Loop Recording (video)]

Video cannot be recorded when the following card combination is used.

–SD memory card or SDHC memory card, and SDXC memory card