- 13. Materials
- Available Recording Time with the Battery

Available Recording Time with the Battery

Listed below are the time lengths available for recording when the battery is being used.

Using an SDHC memory card.

Using the interchangeable lens (H-ES12060).

When outputting via HDMI to an external monitor.

The values listed are approximate.

AG-VBR59

[Rec. File Format]: [MP4]

[Rec Quality] | Continuous available recording time (Actual available recording time) (minutes)
[Image Area of Video]
[FULL] | [PIXEL/PIXEL]
4K/10bit/100M/60p | 270 (135) | —
4K/8bit/100M/30p | 300 (150) | —
FHD/8bit/28M/60p | 300 (150) | 340 (170)

[Rec. File Format]: [MOV]

[Rec Quality] | Continuous available recording time (Actual available recording time) (minutes)
[Image Area of Video]
[FULL] | [PIXEL/PIXEL]
4K/60p/420/10-L | 260 (130) | —
4K/30p/422/10-L | 280 (140) | —
FHD/60p/422/10-L | 280 (140) | 320 (160)
FHD/60p/420/8-L | 300 (150) | 330 (165)

AG-VBR89

[Rec. File Format]: [MP4]

[Rec Quality] | Continuous available recording time (Actual available recording time) (minutes)
[Image Area of Video]
[FULL] | [PIXEL/PIXEL]
4K/10bit/100M/60p | 420 (210) | —
4K/8bit/100M/30p | 480 (240) | —
FHD/8bit/28M/60p | 480 (240) | 530 (265)

[Rec. File Format]: [MOV]

[Rec Quality] | Continuous available recording time (Actual available recording time) (minutes)
[Image Area of Video]
[FULL] | [PIXEL/PIXEL]
4K/60p/420/10-L | 420 (210) | —
4K/30p/422/10-L | 450 (225) | —
FHD/60p/422/10-L | 450 (225) | 500 (250)
FHD/60p/420/8-L | 470 (235) | 520 (260)

AG-VBR118

[Rec. File Format]: [MP4]

[Rec Quality] | Continuous available recording time (Actual available recording time) (minutes)
[Image Area of Video]
[FULL] | [PIXEL/PIXEL]
4K/10bit/100M/60p | 560 (280) | —
4K/8bit/100M/30p | 640 (320) | —
FHD/8bit/28M/60p | 640 (320) | 710 (355)

[Rec. File Format]: [MOV]

[Rec Quality] | Continuous available recording time (Actual available recording time) (minutes)
[Image Area of Video]
[FULL] | [PIXEL/PIXEL]
4K/60p/420/10-L | 560 (280) | —
4K/30p/422/10-L | 600 (300) | —
FHD/60p/422/10-L | 600 (300) | 670 (335)
FHD/60p/420/8-L | 630 (315) | 700 (350)

Actual available recording time is the time available for recording when repeating actions such as turning the camera on and off, starting/stopping recording, etc.

The available recording time vary depending on the surrounding environment and the usage conditions. For example, these will reduce in the following case:

–In low-temperature environments, such as on ski slopes.

If the usage duration drops significantly even when the battery is fully charged, then the battery is at the end of its service life. Check the battery status, and replace with a new battery.