- 11. Menu Guide
- [Custom] menu
- [Custom] menu ([IN/OUT])

[Custom] menu ([IN/OUT])

: Default settings

[HDMI Rec Output]

[Down Convert] | [AUTO] / [4K/30p] ([4K/25p]) / [1080p] / [1080i] / [OFF]
[HDMI Recording Control] | [ON] / [OFF]
[Sound Down Convert] | [AUTO] / [OFF]
[Sound Output (HDMI)] | [ON] / [OFF]
[HDMI MF Assist Output] | [ON] / [OFF]
Sets HDMI output during recording. (HDMI Output Image Quality (Resolution / Frame Rate), HDMI Output Settings)

[SDI Rec Output]

[SDI Output Resolution] | [1080p] / [1080i] / [1080PsF] / [720p]
[SDI Recording Control] | [ON] / [OFF]
[Sound Output (SDI)] | [ON] / [OFF]
[SDI Sound Output Gain Adj.] | [0dB] / [-6dB] / [-8dB]
[SDI MF Assist Output] | [ON] / [OFF]
Sets the SDI output during recording. (SDI output settings) When [System Frequency] is set to [24.00Hz (CINEMA)], [SDI Output Resolution] is fixed to [1080PsF].

[Fan Mode]

[AUTO1] / [AUTO2] / [NORMAL] / [SLOW]
Sets fan operation. [AUTO1]: The fan operation switches automatically according to the temperature of the camera. This setting prioritizes controlling rises in temperature in the camera. [AUTO2]: The fan operation switches automatically according to the temperature of the camera. This setting prioritizes reducing fan noise. [NORMAL]: The fan operates constantly at a standard speed. [SLOW]: The fan operates constantly at low speed.

[Tally Lamp]

[Front Tally Lamp] | [H] / [L] / [OFF]
[Rear Tally Lamp] | [ON] / [OFF]
This sets the operation of the tally lamp.