- 9. Playback
- Playing Back Videos

Playing Back Videos

1Display the playback screen.

Press [].

2Select a video.

Select the image by pressing .

You can move continuously through images by pressing and holding .

Card slot

Video recording time

3Playback the video.

Press .

Elapsed playback time

Playback bar

4Stop playback.

Press .

Operations During Video Playback

Button operation | Description of operation
| Plays / pauses.
| Stops.
| Performs fast-rewind playback. If you press again, the fast-rewind speed increases.
Performs frame-by-frame rewinding (while paused).
| Performs fast-forward playback. If you press again, the fast-forward speed increases.
Performs frame-by-frame forwarding (while paused).

Adjusting volume

Adjust the volume on the connected external device.

To check the sound with headphones (commercially available), connect the headphones to the connected external device.

(While outputting to an external device, audio is not output from the headphone terminal.)

Switching the Card to Display

Images are displayed separately by card slot. When you press [Q.MENU] during playback you can switch the card that will be displayed.

Use the Fn button registered with [Card Slot Change] to operate. In default settings, this is registered in [Q.MENU].

–About Fn buttons (Fn Buttons)

Press [Q.MENU].

Press to select [Card Slot 1] or [Card Slot 2] and then press [MENU/SET].

The camera can playback videos in MP4 and MOV formats.

Video recorded with a [System Frequency] setting that is different to the current one cannot be played back.

When it is output via HDMI and SDI at the same time, it can be output with the same resolution. When [SDI Output] is set to [ON] at [HDMI / SDI Connections] of the [Setup] ([IN/OUT]) menu, output with a resolution above 4K is not possible. When playing back an image at a resolution above 4K, set the [SDI Output] to [OFF].

High resolution audio cannot be output during SDI output.

–When output only via SDI: It is down converted to [48kHz/24bit].

–When output via SDI and HDMI at the same time: It is down converted to [48kHz/24bit] or [48kHz/16bit] depending on the capabilities of the HDMI connection device.

Depending on the aspect ratio, gray bands may be displayed on the top and bottom or the left and right of images. You can change the band color in [Background Color(Playback)] in [HDMI / SDI Connections] of the [Setup] ([IN/OUT]) menu. ([Background Color(Playback)])

Change the settings of your external device if images are displayed with the top or bottom cut off.

Also refer to the operating instructions for the external device.