- 5. Recording settings
- Main Assist Functions
- Color bars / Test Tone

Color bars / Test Tone

The color bars are displayed on the recording screen. A test tone is output while the color bars are being displayed.

[SMPTE] | [EBU] | [ARIB]

[MENU/SET] [] [] Select [Color Bars]

Settings: [SMPTE] / [EBU] / [ARIB]

To end the display, press [MENU/SET].

Adjusting the Test Tone

There are 4 levels ([–12dB], [–18dB], [–20dB], and [MUTE]) of test tone to select.

Rotate to select the test tone level.

The color bars and test tone will be recorded on the video if video recording is started while the color bars are being displayed.