- 3. Basic Operations
- Display Settings
- Information Display (HDMI/SDI)

Information Display (HDMI/SDI)

You can set the output destination of recording information or menu screen. The default setting is set to [AUTO].

[MENU/SET] [] [] Select [Info Display (HDMI/SDI)]

[AUTO] | Only displays to the external device connected via HDMI. When it is not connected via HDMI, it will be displayed on the external device connected via SDI. (when [SDI Output] is [ON]).
[HDMI] | Only displays to the external device connected via HDMI.
[SDI] | Only displays to the external device connected via SDI. (when [SDI Output] is [ON]).
[OFF] | Neither will be displayed.

For external devices not set in the output destination of the information, the whole screen or part of the screen will be displayed in black depending on the setting screen.

By pressing [Fn1], you can switch the settings of [Info Display (HDMI/SDI)] in the order of [AUTO], [HDMI], [SDI], and [OFF].

–[Info Display (HDMI/SDI)] is assigned to the [Fn1] at default setting.

–About Fn buttons (Fn Buttons)

When the menu screen is not output to the external monitor, you can reset the [Info Display (HDMI/SDI)] settings to [AUTO] by pressing [MENU/SET], [Q.MENU], and [Fn3] at the same time.