- 6. Special Video Recording
- Anamorphic Recording
- [Anamorphic Desqueeze Display]

[Anamorphic Desqueeze Display]

Display the desqueezed images suited to the magnification of the anamorphic lens. Using the [Frame Marker], it is also possible to impose on display the frame of the angle of view when cropping after de-squeeze editing.

1Set [Anamorphic Desqueeze Display].

[MENU/SET] [] [] [Anamorphic Desqueeze Display]

Settings: [] (2.0x) / [] (1.8x) / [] (1.5x) / [] (1.33x) / [] (1.30x) / [OFF]

Make settings to suit the magnification of the anamorphic lens you are using.

2Set [Frame Marker].

[MENU/SET] [] [] [Frame Marker] ([Frame Marker])

During recording, images output via HDMI are not displayed de-squeezed.