- 2. Getting Started
- Inserting Cards (Optional)
- Inserting / removing the card

Inserting / removing the card

1Open the card door.

Slide the card door release lever to the direction of the arrow.

2Insert the cards.

Match the orientation of the cards as shown in the figure and then insert them firmly until they click.

Card slot 1

Card slot 2

Do not touch the card connection contacts .

3Close the card door.

The card will be displayed onto the screen of the output destination.

You can set the way to record to card slots 1 and 2:

[] [] [Double Card Slot Function] ([Double Card Slot Function])

Indications during card access

The card access light turns on while the card is being accessed.

Do not perform the following operations during access. The camera may operate incorrectly or the card and recorded images may be damaged.

–Turn off the camera. (Pressing the camera ON/OFF button, stopping power supply, or removing the battery.)

–Remove the card

–Subject the camera to vibration, impacts, or static electricity.

You can set so that the card access light does not turn on:

[] [] [Card Access Light] ([Card Access Light])

Removing a Card

Open the card door.

Push the card until it clicks and then pull the card out straight.

The card may be warm just after the camera has been used.