- 5. Recording settings
- Main Assist Functions
- [Image Stabilizer]

[Image Stabilizer]

Set the image stabilizer operation to match the recording situation.

When using a lens with an O.I.S. switch, set the switch on the lens to ON. When you use a lens with no connection function with the camera, [Image Stabilizer] cannot be selected. When you use a lens without the stabilizer function, [Operation Mode] cannot be selected.

[MENU/SET] [] [] Select [Image Stabilizer]

[Operation Mode] | [Normal]: Corrects vertical, horizontal, and rotational camera shake. This function is suitable for normal recording.
[OFF]: Turns the in-lens image stabilization function OFF.
[E-Stabilization (Video)] | During video recording the 4 types of camera shakes, the vertical, horizontal, pitch, and yaw axes is corrected through the combined use of the in-lens and electronic image stabilizers. When [E-Stabilization (Video)] is working, the [] of the recording screen will be switched to []. When set to [ON], the angle of view may become narrower.

The image stabilizers to be activated differ depending on your lens.

When the following functions are being used, [E-Stabilization (Video)] is not available:

–[Digital Zoom]

–[Variable Frame Rate]

–[Live Cropping]