- 11. Menu Guide
- [Video] menu
- [Video] menu ([Audio])

[Video] menu ([Audio])

: Default settings

[Sound Rec Level Disp.]

[ON] / [OFF]
The sound recording level is displayed on the recording screen. ([Sound Rec Level Disp.])

[Mute Sound Input]

[ON] / [OFF]
This mutes audio input. ([Mute Sound Input])

[Sound Rec Gain Level]

[STANDARD] / [LOW]
This switches the gain of audio input. ([Sound Rec Gain Level])

[Sound Rec Level Adj.]

[MUTE], [-18dB] to [+12dB] ( [0dB])
Manually adjust the sound recording level. ([Sound Rec Level Adj.])

[Sound Rec Level Limiter]

[ON] / [OFF]
The sound recording level is adjusted automatically to minimize sound distortion (crackling noise). ([Sound Rec Level Limiter])

[Wind Noise Canceller]

[HIGH] / [STANDARD] / [OFF]
This reduces the wind noise coming into the built-in microphone while maintaining sound quality. ([Wind Noise Canceller])

[Wind Cut]

[HIGH] / [STANDARD] / [LOW] / [OFF]
This reduces wind noise when an external microphone is connected. (Reduction of Wind Noise)

[Lens Noise Cut]

[ON] / [OFF]
You can reduce the zoom sound produced during video recording when you are using interchangeable lens compatible with power zoom. ([Lens Noise Cut])

[Mic Socket]

[ ] / [ ] / [ ]
Sets the [MIC] terminal input method that suits the device to be connected. (External Microphones (Optional))

[Special Mic.]

[STEREO] / [LENS AUTO] / [SHOTGUN] / [S.SHOTGUN] / [MANUAL]
Sets the sound pickup range when using the Stereo Shotgun Microphone (DMW-MS2: optional). (Setting the Sound Pickup Range (DMW-MS2: Optional))

[XLR Mic Adaptor Setting]

[96kHz/24bit] / [48kHz/24bit] / [48kHz/16bit] / [OFF]
Sets the audio input for when an XLR Microphone Adaptor (DMW-XLR1: optional) is attached. (XLR Microphone Adaptor (Optional))

[Sound Output]

[REALTIME] / [REC SOUND]
Sets the audio output method when headphones are connected. (Switching the Sound Output Method)

[Headphone Volume]

[0] to [LEVEL15] ( [LEVEL3])
Adjusts the volume when headphones are connected. (Adjusting the Headphone Volume)