- 11. Menu Guide
- [Video] menu
- [Video] menu ([Image Format])

[Video] menu ([Image Format])

: Default settings

[Rec. File Format]

[MP4] / [MOV]
Sets the video recording file format. ([Rec. File Format])

[Image Area of Video]

[FULL] / [PIXEL/PIXEL]
Sets the image area during video recording. ([Image Area of Video])

[Rec Quality]

Sets the video recording image quality. ([Rec Quality])

[Rec Quality (My List)]

Calls up a recording quality registered in My List. ([add to list])

[Variable Frame Rate]

[ON] / [OFF]
Varies the recording frame rate to record slow motion video and fast motion video. ([Variable Frame Rate])

[Time Code]

[Time Code Display] | [ON] / [OFF]
[Count Up] | [REC RUN] / [FREE RUN]
[Time Code Value] | [Reset]
[Manual Input]
[Current Time]
[Time Code Mode] | [DF] / [NDF]
[HDMI Time Code Output] | [ON] / [OFF]
[SDI Time Code Output] | [ON] / [OFF]
[External TC Setting] | [TC Synchronization]
[TC Output Reference]
Sets the recording, display, and output of the time code. (Time Code)

[Genlock]

[Genlock Input] | [ON] / [OFF]
[Horizontal Phase Adjustment] | [-206] to [+49] ( [±0])
This synchronizes the image signal of the camera and external device. (Genlock settings)

[Luminance Level]

[0-255] / [16-235] / [16-255]
You can set the luminance range to suit the purpose of video recording. ([Luminance Level])