- Firmware Update
- Firmware Ver. 2.3
- [Focus Ring Control]

[Focus Ring Control]

You can now set the amount of focus movement done by the focus ring on the menu. (When using supported lenses)

[MENU/SET] [] [] Select [Focus Ring Control]

[NON-LINEAR] | Focus responds by accelerating according to rotation speed of the focus ring.
[LINEAR] | Focus responds at a constant amount according to the rotational angle of the focus ring. When using lenses equipped with focus clutch mechanisms, set the lens to AF and the camera to MF.
[SET] | Sets the rotational angle of the focus ring for when [LINEAR] is selected. [90°] to [1080°] / [Maximum]

Angles that cannot be set with the attached lens are not displayed.

For information on lenses that support focus ring control, refer to the following support site:

https://panasonic.jp/support/global/cs/dsc/connect/index.html

(English only)