- 7. Output image
- HDMI Output Image Quality (Resolution / Frame Rate)
- Settings for Down-Converting

Settings for Down-Converting

Make settings for the down-conversion of resolution and frame rate for HDMI output.

[MENU/SET] [] [] [HDMI Rec Output] Select [Down Convert]

[AUTO] | Outputs by down-converting to match the connected device.
[4K/30p] ([4K/25p]) | Outputs by down-converting resolution to 4K and frame rate to either 29.97p or 25.00p.
[1080p] | Down-converts resolution to FHD (1080), and outputs as progressive.
[1080i] | Down-converts resolution to FHD (1080), and outputs as interlaced.
[OFF] | Outputs at the resolution and recording frame rate of the [Rec Quality].

The items you can select depend on the [System Frequency] setting.

Anamorphic (4:3) video is output with a 4K or FHD resolution.

If down-converting, AF may take longer than usual for focusing, and the performance of continuous focus tracking may deteriorate.

Image Quality When Outputting via HDMI

Output is with the resolution and frame rate according to the combinations of the [Rec Quality] and [Down Convert] settings.

When [Down Convert] is set to [AUTO], the output matches the connected device.

[System Frequency]: [59.94Hz (NTSC)]

[Down Convert] | Resolution and recording frame rate of the [Rec Quality]
4K-A/59.94p 4K/59.94p | 4K-A/29.97p 4K/29.97p | 4K-A/23.98p 4K/23.98p
[4K/30p] | 4K/29.97p | 4K/29.97p | ―
[1080p] | 1080/59.94p | 1080/29.97p*1 | 1080/23.98p
[1080i] | 1080/59.94i | 1080/59.94i | ―
[OFF] | 4K/59.94p | 4K/29.97p | 4K/23.98p

*1Output is 1080/59.94p if the connected device is not compatible.

[Down Convert] | Resolution and recording frame rate of the [Rec Quality]
C4K/59.94p | C4K/29.97p | C4K/23.98p
[4K/30p] | 4K/29.97p | 4K/29.97p | ―
[1080p] | 1080/59.94p | 1080/29.97p*1 | 1080/23.98p
[1080i] | 1080/59.94i | 1080/59.94i | ―
[OFF] | C4K/59.94p | C4K/29.97p | C4K/23.98p

*1Output is 1080/59.94p if the connected device is not compatible.

[Down Convert] | Resolution and recording frame rate of the [Rec Quality]
1080/59.94p | 1080/29.97p | 1080/23.98p
[4K/30p] | ― | ― | ―
[1080p] | 1080/59.94p | 1080/29.97p*1 | 1080/23.98p
[1080i] | 1080/59.94i | 1080/59.94i | ―
[OFF] | 1080/59.94p | 1080/29.97p | 1080/23.98p

*1Output is 1080/59.94p if the connected device is not compatible.

[System Frequency]: [50.00Hz (PAL)]

[Down Convert] | Resolution and recording frame rate of the [Rec Quality]
4K-A/50.00p 4K/50.00p | 4K-A/25.00p 4K/25.00p | C4K/50.00p | C4K/25.00p
[4K/25p] | 4K/25.00p | 4K/25.00p | 4K/25.00p | 4K/25.00p
[1080p] | 1080/50.00p | 1080/25.00p*2 | 1080/50.00p | 1080/25.00p*2
[1080i] | 1080/50.00i | 1080/50.00i | 1080/50.00i | 1080/50.00i
[OFF] | 4K/50.00p | 4K/25.00p | C4K/50.00p | C4K/25.00p

*2Output is 1080/50.00p if the connected device is not compatible.

[Down Convert] | Resolution and recording frame rate of the [Rec Quality]
1080/50.00p | 1080/25.00p
[4K/25p] | ― | ―
[1080p] | 1080/50.00p | 1080/25.00p*2
[1080i] | 1080/50.00i | 1080/50.00i
[OFF] | 1080/50.00p | 1080/25.00p

*2Output is 1080/50.00p if the connected device is not compatible.

[System Frequency]: [24.00Hz (CINEMA)]

[Down Convert] | Resolution and recording frame rate of the [Rec Quality]
4K-A/24.00p 4K/24.00p | C4K/24.00p | 1080/24.00p
[1080p] | 1080/24.00p | 1080/24.00p | 1080/24.00p
[OFF] | 4K/24.00p | C4K/24.00p | 1080/24.00p