- 2. Getting Started
- Connecting the external monitor
- Attaching the Cable Lock Band

Attaching the Cable Lock Band

Use of the supplied cable lock band prevents detachment of the cable and damage to the terminals.

Put the camera on a stable surface to perform this task.

1Loosely mount the cable lock band to the cable lock band mount on the camera, and then rotate the screws in the direction of the arrows to secure the cable lock band.

2Connect the AC adaptor, the HDMI cable and the USB connection cable to the camera.

3Fit the AC cable to the clamp.

4Fit the HDMI cable and USB connection cable to the clamp.

Removing the cable lock band

To remove the cable lock band, follow the steps for attaching it in the reverse order.

It may not be possible to attach HDMI cables or USB connection cables depending on the shape.