- 4. Recording Videos
- Synchronizing the Time Code with an External Device
- Preparations for Time Code Synchronization

Preparations for Time Code Synchronization

When [Count Up] is set to [FREE RUN], you can synchronize the initial value of the time code with an external device.

[TC IN/OUT] terminal

BNC cable (commercially available)

External devices

1Set [Count Up] to [FREE RUN].

[MENU/SET] [] [] [Time Code] [Count Up] [FREE RUN]

2Connect the camera and external device with a BNC cable.

When connecting a BNC cable to the [TC IN/OUT] terminal, use one that is less than 2.8 m (9.1 feet).

It is recommended to use a double shielded BNC cable equivalent to 5C-FB.