- 2. Getting Started
- Power supply

Power supply

You can supply power to the camera using an AC adaptor (supplied), a PoE+*1 compatible switching hub or PoE+ compatible injector (commercially available), and a battery pack (optional)*2.

*1PoE+ is an abbreviation of Power Over Ethernet Plus.

*2This will be referred to as “battery pack” or “battery” onwards.

When several power supplies are connected at the same time, it will be prioritized in the order of AC adaptor, PoE+ power supply and then battery.

The battery that can be used with the camera is AG-VBR59/AG-VBR89/AG-VBR118. (As of October 2020)

Supplying power with an AC adaptor
Supplying power from a PoE+ power supply
Turning the camera on
Turning the camera off
Power Indications