- 13. Materials
- External Monitor Displays
- Recording Screen

Recording Screen

AWBc AWBw | [White Balance] (White Balance (WB))
| White balance adjustment (Adjusting the White Balance)
| [Photo Style] ([Photo Style])
| [Filter Settings] ([Filter Settings]) / Filter effect adjustment (Adjusting the Filter Effect)
| LUT View Assist ([V-Log L View Assist])
| [HLG View Assist] ([HLG View Assist])
MP4 MOV | [Rec. File Format] ([Rec. File Format])
FHD 420/8-L | [Rec Quality] ([Rec Quality])
59.94p 60/59.94p | Recording frame rate ([Rec Quality]) / [Variable Frame Rate] ([Variable Frame Rate])
| [Image Area of Video] ([Image Area of Video])
AF MF | [Focus Mode] (Selecting the Focus Mode, Record Using MF)
AFL | AF Lock (Locking Focus and Exposure (AF/AE Lock))
| [Focus Peaking] ([Focus Peaking])
| [AF Mode] (Selecting the AF Mode)
| Wi-Fi connection status (Checking operation when connected to a network)
| Wired LAN connection status (Checking operation when connected to a network)
| USB connection status (“LUMIX Tether”) (Tethered Recording)
| Bluetooth connection status (Checking operation when connected to a network)
| [Location Logging] ([Location Logging])
| [Image Stabilizer] ([Image Stabilizer])
| Jitter warning
| [Anamorphic Desqueeze Display] ([Anamorphic Desqueeze Display])
| [Loop Recording (video)] ([Loop Recording (video)])
| [Digital Zoom] ([Digital Zoom])

| [Histogram] ([Histogram])
| AF area
| Spot-metering target ([Metering Mode])
| [Center Marker] ([Center Marker])
[Level Gauge] ([Level Gauge])

XXmXXs | Elapsed recording time (Screen Displays While Video Recording)
TC 00:00:00.00 | Time code (Time Code)
| Built-in microphone, External microphone ([Sound Rec Level Disp.], External Microphones (Optional))
48kHz/16bit | [XLR Mic Adaptor Setting] (XLR Microphone Adaptor (Optional))
| [Sound Rec Level Limiter] ([Sound Rec Level Limiter])
| Mute ([Mute Sound Input])
Sound recording level ([Sound Rec Level Disp.])
| Temperature rise warning icon (Recording)
| Fan error warning icon (Others)

2021.12. 1 10:00:00 | [Time Stamp Rec.] ([Time Stamp Rec.])
| Recording state (lit in red) (Screen Displays While Video Recording)
| [Exposure Mode] ([Exposure Mode]), Recording mode ([Rec Mode] menu (Recording mode))
| [Metering Mode] ([Metering Mode])
AEL | [AE LOCK] (Locking Focus and Exposure (AF/AE Lock))
250 | Shutter speed
F2.8 | Aperture value
| [Exposure Comp.] (Exposure Compensation)
| Manual exposure assist (Manual Exposure Assist)
| [Sensitivity] (ISO Sensitivity) / [Dual Native ISO Setting] ([Dual Native ISO Setting])
| Card access indication (lit in red) (Screen Displays While Video Recording)
| Card slot (Inserting Cards (Optional)) / [Double Card Slot Function] ([Double Card Slot Function])
| No card
| Card full
XXmXXs | Video recording time (Screen Displays While Video Recording)
| Battery indication (Battery indication) Power supply (Power supply)

Control Panel

| Frame rate ([Rec Quality]) / [Variable Frame Rate] ([Variable Frame Rate])
| Shutter speed
| Aperture value

| [Exposure Mode] ([Exposure Mode]), Recording mode ([Rec Mode] menu (Recording mode))
| Exposure compensation value (Exposure Compensation) / Manual exposure assist (Manual Exposure Assist)
| [Image Area of Video] ([Image Area of Video])
| Time code (Time Code)
| Recording state (Screen Displays While Video Recording)

| [Rec. File Format] ([Rec. File Format]) / [Rec Quality] ([Rec Quality])
| Card slot (Inserting Cards (Optional)) / [Double Card Slot Function] ([Double Card Slot Function])
24m59s | Video recording time (Screen Displays While Video Recording)
| Wi-Fi connection status (Checking operation when connected to a network)
| Wired LAN connection status (Checking operation when connected to a network)
| USB connection status (“LUMIX Tether”) (Tethered Recording)
| Bluetooth connection status (Checking operation when connected to a network)
| [Fan Mode] ([Fan Mode])
| Battery indication (Battery indication) Power supply (Power supply)

| Built-in microphone, External microphone ([Sound Rec Level Disp.], External Microphones (Optional))
48kHz/16bit | [XLR Mic Adaptor Setting] (XLR Microphone Adaptor (Optional))
| [Sound Rec Level Limiter] ([Sound Rec Level Limiter])
| Mute ([Mute Sound Input])
Sound recording level ([Sound Rec Level Disp.])

| [Sensitivity] (ISO Sensitivity) / [Dual Native ISO Setting] ([Dual Native ISO Setting])
| [Photo Style] ([Photo Style])
| LUT View Assist ([V-Log L View Assist]) / [HLG View Assist] ([HLG View Assist])
| [White Balance] (White Balance (WB))