- 5. Recording settings
- Metering / Exposure / ISO Sensitivity
- Exposure Compensation

Exposure Compensation

You can compensate the exposure when the correct exposure determined by the camera is too bright or too dark.

You can adjust the exposure in 1/3 EV steps in a range of ±3 EV.

1Display the exposure compensation screen.

[MENU/SET] [] [] [Exposure Comp.]

2Compensate the exposure.

Rotate .

3Confirm your selection.

Press [MENU/SET].

If you set the ISO sensitivity to [AUTO] when [Exposure Mode] is set to [M], you can compensate the exposure.

The set exposure compensation value is stored even if you turn off the camera.

The standard value for correct exposure can be adjusted:

[] [] [Exposure Offset Adjust.] ([Exposure Offset Adjust.])