- 4. Recording Videos
- Recording Videos
- Recording Videos

Recording Videos

1Start recording.

Press the video rec. button .

Release the video rec. button right after you press it.

During video recording, the front tally lamp and rear tally lamp light.

2Stop recording.

Press the video rec. button again.

Screen Displays While Video Recording

The video recording time and elapsed recording time will be displayed.

The recording state indication and card access indication turn red while videos are being recorded.

When the remaining capacity of the battery or card gets low during video recording, the tally lamps blink at long intervals. When there is no remaining capacity in the battery or card, video recording is stopped and the tally lamps blink at short intervals.

If an operation such as a zoom or button operation is performed during video recording, that operation sound may be recorded.

The lens operation sound (AF and image stabilizer) may be recorded to video.

If the operation sound of pressing the video rec. button to end recording bothers you, try the following:

–Record by remotely operating the camera (12. Remote Operations)

–Connect a remote control unit (commercially available) that is compatible with the camera to the [REMOTE] terminal to record.

Depending on the type of card, the card access indication may appear for a while after video recording. This is not a malfunction.

Depending on the external device, during playback, situations such as image or sound quality being poor, recording information not being displayed correctly, or playback not being possible may occur.

If the camera temperature rises, [] may be displayed and recording may stop. Wait until the camera cools down.

You can change the tally lamp that turns on. You can also change the settings so the tally lamps do not turn on:

[] [] [Tally Lamp] ([Tally Lamp])

You can display a red frame on the recording screen that indicates that video is being recorded:

[] [] [Red REC Frame Indicator] ([Red REC Frame Indicator])