- 6. Special Video Recording
- [Segmented File Recording]

[Segmented File Recording]

To avoid video loss due to unforeseen interruptions to the power supply, recorded video is divided every few minutes while MOV video is being recorded.

The divided videos are saved as one group image.

1Set [Rec. File Format] to [MOV].

[MENU/SET] [] [] [Rec. File Format] [MOV]

2Set [Segmented File Recording].

[MENU/SET] [] [] [Segmented File Recording] [10MIN.] / [5MIN.] / [3MIN.] / [1 MIN.]

When the following function is being used, [Segmented File Recording] is not available:

–[Loop Recording (video)]