- Firmware Update
- Firmware Ver. 2.3
- Models Supporting Output of RAW Video Data Have Been Added

Models Supporting Output of RAW Video Data Have Been Added

RAW Video Data of this camera can now be recorded to a Blackmagic Design external recorder.

Recording of the RAW Video Data of this camera has been confirmed on the following external recorder. (As of October 2021)

–Blackmagic Design “Blackmagic Video Assist 5″ 12G HDR” and “Blackmagic Video Assist 7″ 12G HDR” (Ver. 3.5 or higher)
For details, please contact Blackmagic Design.

This does not guarantee all of the capabilities that the compatible external recorder may have.

You will need compatible software to edit the RAW Video Data recorded with the external recorder.

Visit the following site to download LUT data or view the latest support information:

https://panasonic.jp/support/global/cs/dsc/

(English only)

Video cannot be recorded to cards while RAW Video Data is being output via HDMI.

When [System Frequency] is set to [24.00Hz (CINEMA)], RAW Video Data cannot be output via HDMI.

Refer to “Support for Output of RAW Video Data” in “Firmware Ver. 2.0” for operations and limitations for RAW Video Data output. (Support for Output of RAW Video Data)