- 4. Recording Videos
- Recording Settings For Video
- [System Frequency]

[System Frequency]

This changes the system frequency of videos that are recorded and played back.

The default setting is for the system frequency to be set to the TV broadcast system for the region where the camera was bought.

[MENU/SET] [] [] Select [System Frequency]

[59.94Hz (NTSC)] | System frequency for regions using the NTSC broadcasting system
[50.00Hz (PAL)] | System frequency for regions using the PAL broadcasting system
[24.00Hz (CINEMA)] | System frequency for producing cinema film

After changing the setting, turn the camera off and on.

If you record using a system frequency that differs from the broadcasting system of your region, it may not be possible for you to properly playback videos on your TV.

A video recorded with a system frequency different from the setting of [System Frequency] cannot be played back in the camera.