- 12. Remote Operations
- Operating the Camera with a Smartphone
- [Remote Wakeup]

[Remote Wakeup]

Even when the camera is turned off, the smartphone can be used to start the camera and record images, or check the recorded images.

Preparation:

Enable [Remote Wakeup] on the camera.

[MENU/SET] [] [] [Bluetooth] [Remote Wakeup] [ON]

[Remote Wakeup] is not available when connected with a LAN cable.

Turning Off the Camera

Select [] ([Remote shooting]) or [] ([Import images]) in the “LUMIX Sync” home screen.

Select [ ] in the “LUMIX Sync” home screen.

Select [Turn off the camera].

[Turn off the camera] is not displayed when it is not connected via Wi-Fi.

Select [Power OFF].

When [Remote Wakeup] has been set, since the Bluetooth function continues to work even when the camera is turned off, power is being consumed.

If you turn off the camera by pressing the camera ON/OFF button on the camera, [Remote Wakeup] will not work.

Turning On the Camera

Select [] ([Remote shooting]) in the “LUMIX Sync” home screen.

(iOS devices) When a message to confirm the change of destination is displayed, select [Join].

The camera turns on, and automatically connects using Wi-Fi.

Shortening the Return Time when performing [Remote Wakeup]

You can shorten the time it takes to enable the priority function when waking up the camera remotely.

Preparation:

Set [Remote Wakeup] in [Bluetooth] to [ON].

[MENU/SET] [] [] [Bluetooth] Select [Returning from Sleep Mode]

[Import / Remote Priority] | Shortens the time to return when using [Import images] or [Remote shooting].
[Remote Shutter Priority] | Shortens the time to return when using [Shutter Remote Control].