- 4. Recording Videos
- Recording Settings For Video
- [Image Area of Video]

[Image Area of Video]

Set the image area during video recording. The angle of view differs depending on the image area. Narrowing the image area allows you to achieve a telescopic effect without image deterioration.

[MENU/SET] [] [] Select [Image Area of Video]

Item | Settings details
[FULL] | Records according to the range that corresponds to the image circle of the lens that is for Micro four thirds. Angle of view: Wide Telescopic effect: Not possible
[PIXEL/PIXEL] | Records with one pixel on the sensor, which is equal to one pixel of the video. Records a range corresponding to the resolution range in [Rec Quality]. ([Rec Quality]) Angle of view: Narrow Telescopic effect: Possible

Image area (Ex.: FHD video)

When the following functions are being used, [Image Area of Video] is fixed to [FULL].

–[Live Cropping]

–Anamorphic (4:3) video

–C4K video

–4K video