- 10. Camera Customization
- Fn Buttons
- Register Functions to the Fn Buttons

Register Functions to the Fn Buttons

1Select [Fn Button Set].

[MENU/SET] [] [] [Fn Button Set] [Setting in REC mode] / [Setting in PLAY mode]

2Select the button.

Press to select the button and then press [MENU/SET].

Selection is also possible by rotating .

3Find the function to register.

You can select by pressing to select the sub tab, pressing or rotating , and then pressing .

Each press [Q.MENU] switches between tabs [1] and [2].

4Register the function.

Press to select a function and then press [MENU/SET].

Selection is also possible by rotating .

Select items with [] by selecting the item again.

Depending on the button, some functions cannot be registered.

You can also press and hold the Fn button (2 sec.) to display the screen in Step 4. (This may not be displayed depending on the registered function and on the button type.)

Setting Items ([Fn Button Set] / [Setting in REC mode])

[1] tab

[Image Quality]

[Exposure Mode] ([Exposure Mode])

[Aperture Value] ([Exposure Mode])

[Shutter Speed] ([Exposure Mode])

[Exposure Comp.] (Exposure Compensation)

[Dual Native ISO Setting] ([Dual Native ISO Setting])

[Sensitivity] (ISO Sensitivity)

[White Balance] (White Balance (WB))

[Photo Style] ([Photo Style])

[Metering Mode] ([Metering Mode])

[i.Dynamic Range] ([i.Dynamic Range])

[Filter Effect] ([Filter Settings])

[One Push AE]

–Adjusts the aperture value and shutter speed to the settings suited for the correct exposure determined by the camera.

[Synchro Scan] ([Synchro Scan])

[Focus]

[Focus Mode] (Selecting the Focus Mode)

[AF Mode] (Selecting the AF Mode)

[AF Custom Setting(Video)] ([AF Custom Setting(Video)])

[Focus Peaking] ([Focus Peaking])

[Focus Peaking Sensitivity] ([Focus Peaking Sensitivity])

[1-Area AF Moving Speed] ([1-Area AF Moving Speed])

[Focus Ring Lock] ([Focus Ring Lock])

[AE LOCK] (Locking Focus and Exposure (AF/AE Lock))

[AF LOCK] (Locking Focus and Exposure (AF/AE Lock))

[AF/AE LOCK] (Locking Focus and Exposure (AF/AE Lock))

[AF-ON]

–AF works.

[AF-ON : Near Shift]

–AF operates giving priority to close-up subjects.

[AF-ON : Far Shift]

–AF operates giving priority to distant subjects.

[Focus Area Set]

–Displays the AF area/MF Assist transition screen.

[Image Format]

[Rec. File Format] ([Rec. File Format])

[Rec Quality] ([Rec Quality])

[Rec Quality (My List)] ([add to list])

[Variable Frame Rate] ([Variable Frame Rate])

[Time Code Display] ([Time Code Display])

[Audio]

[Sound Rec Level Disp.] ([Sound Rec Level Disp.])

[Mute Sound Input] ([Mute Sound Input])

[Sound Rec Level Adj.] ([Sound Rec Level Adj.])

[Sound Rec Level Limiter] ([Sound Rec Level Limiter])

[XLR Mic Adaptor Setting] (XLR Microphone Adaptor (Optional))

[Special Mic. Directivity Adjust] (Setting the Sound Pickup Range (DMW-MS2: Optional))

[Others (Video)]

[Image Stabilizer] ([Image Stabilizer])

[E-Stabilization (Video)] ([E-Stabilization (Video)])

[Image Area of Video] ([Image Area of Video])

[Digital Zoom] ([Digital Zoom])

[Focus Transition] ([Focus Transition])

[Live Cropping] ([Live Cropping])

[Operation]

[Q.MENU] (Quick Menu)

[Rec / Playback Switch]

–Switches to the playback screen.

[Video Record] (Recording Videos)

[Cursor Button Lock]

–Disables the operation of cursor buttons and [MENU/SET]. Pressing the Fn button assigned with [Cursor Button Lock] again will release the lock.

[Display Information] (Switch the information display with a Fn button, Displaying Descriptions About Menu Items and Settings)

[2] tab

[Monitor / Display]

[Level Gauge] ([Level Gauge])

[Histogram] ([Histogram])

[Luminance Spot Meter] ([Luminance Spot Meter])

[Frame Marker] ([Frame Marker])

[Zebra Pattern] ([Zebra Pattern])

[LUT View Assist (HDMI)] ([LUT View Assist (HDMI)])

[LUT View Assist (SDI)] ([LUT View Assist (SDI)])

[LUT Select] ([LUT Select])

[HLG View Assist (HDMI)] ([HLG View Assist])

[HLG View Assist (SDI)] ([HLG View Assist])

[Anamorphic Desqueeze Display] ([Anamorphic Desqueeze Display])

[Color Bars] (Color bars / Test Tone)

[Lens / Others]

[Zoom Control]

–You can operate zoom when using an interchangeable lens that supports the power zoom.

[Step Zoom] ([Step Zoom])

[Card/File]

[Destination Card Slot]

–Changes the priority of cards for recording. This can be used if [Double Card Slot Function] ([Double Card Slot Function]) is set to [Relay Rec].

[IN/OUT]

[LAN / Wi-Fi] ([LAN / Wi-Fi])

[Info Display (HDMI/SDI)] (Information Display (HDMI/SDI))

[Fan Mode] ([Fan Mode])

[Others]

[No Setting]

–Set when not using as a Fn button.

[Off (Disable Press and Hold)]

–This sets the registration screen of the function to not be displayed even when you long press the Fn button.

[Restore to Default]

–Restore the default settings for the Fn button. (Fn Button Default Settings)

Setting Items ([Fn Button Set] / [Setting in PLAY mode])

[1] tab

[Playback Mode]

[Anamorphic Desqueeze Display] ([Anamorphic Desqueeze Display])

[Add/Delete Info.]

[Delete Single] ([Delete Single])

[Protect] ([Protect])

[Rating1] ([Rating])

[Rating2] ([Rating])

[Rating3] ([Rating])

[Rating4] ([Rating])

[Rating5] ([Rating])

[Edit Image]

[Copy] ([Copy])

[Operation]

[Rec / Playback Switch]

–Switches to the recording screen.

[Video Record] (Recording Videos)

[Display Information] (Switch the information display with a Fn button, Displaying Descriptions About Menu Items and Settings)

[Card/File]

[Card Slot Change] (Switching the Card to Display)

[IN/OUT]

[LAN / Wi-Fi] ([LAN / Wi-Fi])

[Info Display (HDMI/SDI)] (Information Display (HDMI/SDI))

[Fan Mode] ([Fan Mode])

[LUT View Assist (HDMI)] ([LUT View Assist (HDMI)])

[LUT View Assist (SDI)] ([LUT View Assist (SDI)])

[HLG View Assist (HDMI)] ([HLG View Assist])

[HLG View Assist (SDI)] ([HLG View Assist])

[Others]

[No Setting]

–Set when not using as a Fn button.

[Off (Disable Press and Hold)]

–This sets the registration screen of the function to not be displayed even when you long press the Fn button.

[Restore to Default]

–Restore the default settings for the Fn button. (Fn Button Default Settings)