- 11. Menu Guide
- [Video] menu
- [Video] menu ([Others])

[Video] menu ([Others])

: Default settings

[Image Stabilizer]

[Operation Mode] | [] / [OFF]
[E-Stabilization (Video)] | [ON] / [OFF]
Configures image stabilizer settings. ([Image Stabilizer])

[Digital Zoom]

[4x] / [2x] / [OFF]
You can zoom in up to 4x the original zoom magnification. ([Digital Zoom])

[Focus Transition]

[Start]
[Focus Pull Setting] | [1] / [2] / [3]
[Focus Transition Speed] | [SH] / [H] / [M] / [L] / [SL]
[Focus Transition Rec] | [1] / [2] / [3] / [OFF]
[Focus Transition Wait] | [10SEC] / [5SEC] / [OFF]
Smoothly transitions the focus position from the current position to a position registered in advance. ([Focus Transition])

[Loop Recording (video)]

[ON]/ [OFF]
When the recording fills the card to capacity, recording continues while deleting older data. ([Loop Recording (video)])

[Segmented File Recording]

[10MIN.] / [5MIN.] / [3MIN.] / [1 MIN.] / [OFF]
Video is divided every few minutes while being recorded. ([Segmented File Recording])

[Live Cropping]

[40SEC] / [20SEC] / [OFF]
By cropping a part of the range displayed in the live view, it is possible to record FHD video that incorporates panning and zooming with the camera staying in a fixed position. ([Live Cropping])

[Time Stamp Rec.]

[ON] / [OFF]
Records the recorded date and time superimposed on the images. You cannot delete recording dates after superimposing them. When the following functions are being used, [Time Stamp Rec.] is not available: –Anamorphic (4:3) video –[Variable Frame Rate]