- 5. Recording settings
- Metering / Exposure / ISO Sensitivity
- [Luminance Level]

[Luminance Level]

You can set the luminance range to suit the purpose of video recording.

[MENU/SET] [] [] Select [Luminance Level]

Settings: [0-255] / [16-235] / [16-255]

When set to a 10-bit [Rec Quality], the setting items change to [0-1023], [64-940], and [64-1023].

When [Photo Style] is set to [V-Log L], this is fixed to [0-255] ([0-1023]).