- 10. Camera Customization
- Quick Menu Customization
- Register to the Quick Menu

Register to the Quick Menu

Change the menus to be displayed in the Quick menu.

1Select [Q.MENU Settings].

[MENU/SET] [] [] [Q.MENU Settings] [Item Customize (Video)]

2Select the item position ( to ).

Press to select the position and then press [MENU/SET].

3Find the function to register.

You can select by pressing to select the sub tab, pressing or rotating , and then pressing .

Each press of [Q.MENU] switches between tabs [1] and [2].

4Register menu items.

Press to select an item and then press [MENU/SET].

Selection is also possible by rotating .

Select items with [] by selecting the item again.

Menu Items That Can Be Registered

[1] tab

[Image Quality]

[Exposure Mode] ([Exposure Mode])

[Aperture Value] ([Exposure Mode])

[Shutter Speed] ([Exposure Mode])

[Exposure Comp.] (Exposure Compensation)

[Dual Native ISO Setting] ([Dual Native ISO Setting])

[Sensitivity] (ISO Sensitivity)

[White Balance] (White Balance (WB))

[Photo Style] ([Photo Style])

[Metering Mode] ([Metering Mode])

[i.Dynamic Range] ([i.Dynamic Range])

[Filter Effect] ([Filter Settings])

[Synchro Scan] ([Synchro Scan])

[Focus]

[Focus Mode] (Selecting the Focus Mode)

[AF Mode] (Selecting the AF Mode)

[AF Custom Setting(Video)] ([AF Custom Setting(Video)])

[Focus Peaking] ([Focus Peaking])

[Focus Peaking Sensitivity] ([Focus Peaking Sensitivity])

[1-Area AF Moving Speed] ([1-Area AF Moving Speed])

[Image Format]

[Rec. File Format] ([Rec. File Format])

[Rec Quality] ([Rec Quality])

[Rec Quality (My List)] ([add to list])

[Variable Frame Rate] ([Variable Frame Rate])

[Time Code Display] ([Time Code Display])

[Audio]

[Sound Rec Level Disp.] ([Sound Rec Level Disp.])

[Sound Rec Level Adj.] ([Sound Rec Level Adj.])

[Sound Rec Level Limiter] ([Sound Rec Level Limiter])

[XLR Mic Adaptor Setting] (XLR Microphone Adaptor (Optional))

[Special Mic. Directivity Adjust] (Setting the Sound Pickup Range (DMW-MS2: Optional))

[Others (Video)]

[Image Stabilizer] ([Image Stabilizer])

[E-Stabilization (Video)] ([E-Stabilization (Video)])

[Image Area of Video] ([Image Area of Video])

[Digital Zoom] ([Digital Zoom])

[Focus Transition] ([Focus Transition])

[Live Cropping] ([Live Cropping])

[Monitor / Display]

[Level Gauge] ([Level Gauge])

[Histogram] ([Histogram])

[Luminance Spot Meter] ([Luminance Spot Meter])

[Frame Marker] ([Frame Marker])

[Zebra Pattern] ([Zebra Pattern])

[LUT View Assist (HDMI)] ([LUT View Assist (HDMI)])

[LUT View Assist (SDI)] ([LUT View Assist (SDI)])

[HLG View Assist (HDMI)] ([HLG View Assist])

[HLG View Assist (SDI)] ([HLG View Assist])

[Anamorphic Desqueeze Display] ([Anamorphic Desqueeze Display])

[Color Bars] (Color bars / Test Tone)

[2] tab

[Lens / Others]

[Step Zoom] ([Step Zoom])

[Card/File]

[Destination Card Slot]

–Changes the priority of cards for recording. This can be used if [Double Card Slot Function] ([Double Card Slot Function]) is set to [Relay Rec].

[IN/OUT]

[LAN / Wi-Fi] ([LAN / Wi-Fi])

[Fan Mode] ([Fan Mode])

[Others]

[No Setting]

–Set when not registering any function.

Quick Menu Detailed Settings

[MENU/SET] [] [] Select [Q.MENU Settings]

[Layout Style] | Changes the appearance of the Quick menu. [MODE1]: Displays the live view and the menu simultaneously. [MODE2]: Displays the menu in full screen.
[Item Customize (Video)] | Customizes the Quick menu to display.